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How to retrieve fault codes:

If you wish to view the fault codes your ACC unit has stored, simply hold down the AUTO and OFF buttons
on the ACC control panel

The display will then display a single digit number on the left. and a double digit on the right

ie1___ 21

This would signify 1 fault code stored, code 21

Clicking on the tech 2 code will show a brief description of the fault, use browers back button to retum,

12 Stepping motor, air distribution flap  Short-circuit to ground B2400
13 Stepping motor, air distribution flap  Jammed flap 82406
14 Stepping motor, air distribution flap  Loose flap 82405
18 Heat exchanger solencid Open circuit, short-circuit to ground 82375
18 Heat exchanger solenoid Short-circuit to B+ B2375 |
19 Circulation pump Open circuit, short-circuit to ground 82380 ¥,
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Este es el código








