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@ EARE Parts & Service Information

Subject:  High Temperature Gauge Reading  szeror———5
3
Application: 1991~ 900 Models with B212 Engine -
s |

03/92-0191 |

With tho inroduction o tho 2.1 lter (B212) naurally aspirated sngins In 1991 modal yoar 300 and 9008 models,
he cooing fan circut was changed compared o the 2.0 iar angina. Whan the B212 engina codlanttamparars
tises 1o the spacified avelonly the main coaling fan comes onfhe ATC s swiehed of. 1fiho A/C s swihad or.
bath the main cocling fan an the AIC cooiing fan aperats, This ifers rom th provicus fan wiring lagic wnerd
bots ans angaged when tho engine tomparaturo reached tho spacied level regardiass of he st of the A/C
swch

In cortain driving condiions iy Giing, AIG it o), this may causa the dasriboard tamperature gauge o reac
justsolow thorad zono. Whil ths s ntIndeaive o an verhoating stuaton, t ray bo ¢ausa fo some customer

e coolng system is working s designed and i provkding adeduato ongine cooling. Howaver, f cusiomar s
prona o ancauntering tistype af drving contiton and i not comforabla i he GaUge reading, the caoling fan
iing cicult can 5a rowired so that bt fans ongage wihor the AIC boing sctvate.

Parts Required
Raay PSS T2 190
Fuse Box Pin PNTe7i 708
18 gauge wire local supply

Spiso Connostor oS 59 998
Spics Connactor PiNSS 50 004

Coaling Fan Circuit Rewiring Procedura

1. Discannectthe ground cable fom the battry 4. insall the Cartor rlay 85 72 180 into peston

2. Unplug the Bosch relay from positon I of the 5, Reconnest the ground cabl f the Battr.
main fso box (s Bosch rolay s no longor

=) 6. Chock tho systom function. Both coaling fans
3. Regositon the pins in the relay sacket 5o thay should come on fhe AIG s swiched on or i the
match the configuration of Carte relay P/N 85 72 ngine coolant temperaturo gets warm anough &
90: ongage tho cooling fan without the AIC engaged.

Ax Wiro 113A (plack 0.Smm) — positon 86 Referance the ravised viring diagram on the back or

this buloin o s00 how the wiring should ook afe -

B.. Wiro 114 (whito 2Smim) — posison 87 o er b oaicudiviing

€. Wira 116 {lus 0.5mm) | 146C (yelowrod
28mm = poskion 30 Warranty Information:
0. Wire 408 e 0.75mm) — positen &5 ifacustomer complaintrequires his towiing, youray
s )= pe submi & caim s Fairs - Code
o tocal suppics wro must bo acded o I5544—51-0-01-05. Time Alowance s 0.5 hours
oo e el e e 111 which shuid be stared as stight .
{arwon) fom o7 ofroia 166 oundin s
oo &
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