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If you have problems with this bulletin's instructions, you can simply wire the 310 relay in so that +30 (power all the time) is on pin 30 of the relay, that the wire going to the fan is on pin 87 of the relay and pin 85 is either jumped from +30 ( fan will run with key off as long as the fan sensor is closed (hot engine)) or +15 ( power with the key on) ( fan will run with key on and fan sensor closed) and pin 86 connected to the blue wire from the fan sensor.
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Subject: Radiator Fan Time-Delay Relay

Application: 1989~ 900 and 9000 Models

Etectrical
= a3
3 38
02/93-0305 an

Supersedes 06/92-0218

On Gertain 900 and 500D cars,the fan may ot shutoff afer the 10 minute cool down pariod and n some cases,
causos e battery 1o go doad, Thersfore, producion o tho tme-delay relay, /N 95 63 333, for the radiator fan has
Eoon disoontimuad. 18 suparsedad by ino standard alay, PIN 85 22 310. On 1990 mocis, tese releys are uly
nlofthangesble and the Siandard rlay. PIN 85 22 310, should be intalled as  replapemen pa, W needod

Sorme 1969 9000 modelcars do not have the jurmpar connotion Which supplies n relay coil with operating curtant
omtorminal 86, His aasy tocheok whathorof ok car as tis umper connection b follwing he procedure described
Selowt I 2 standrd reay 1 fied 1o  car wihout tis fumper. the fan wil notfunction and the engin vl overhezt.

Cars Affecte

900 Models,  VIN M2500000—
VIN M5010548—

VIN M7019457-
9000 Modsle, VIN M102022-
Parts:

Standard Folay 8522310

“Tog olowing par are for 8000 Only

Cable, yalow. 0.5 mm? 50 - 60 mm long

Cavle, g, 25 - 40 e 9120791

Cavle,ug, 0.5 - 1.0 8120775
Oisassombly ool 8580 094 (or smilar)
Grmping plers 2014 222 (or similar)

Action:
200 Mosels
ot ocation oftha tme-delay relay efor fo Figure 1

Replace oid time-dolay rlay with new standard reay.
a5 nesdiad. No modifcations arc requied.

2000 Mosels

Check for Jumper (8000 oniy), Figure 2.
Checkewhether acable lugis fited at elay pastion £
ot the radiator fan (ow spsed), torminai 86. 1 5o, it
& new standard olay

1170 cabl lug i ited. a jurper sonncction must be
atangod between terminals 30 and 85 as described
Eelow for 9000 model.

Figure 1. Time-Delay Aoy, Radiator
Fan—900 bogel

Figure 2. Check for Jumpor (5000)
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W Installation Prooedures -~ 3000.

1. Disconnact the positve battery cable from the
battery orminal o prevent shoring.

2. Ramove the front relay and fuss board from the
protective box.

3. Withoraw the wiing hamess by a suffcent
amount to allow acoess 1o the underside of tha
relay board, Figure 3.

Figure 3. Underside of Felay Board (3000)

4. Disconnect the yallow 40 ram? cable at relay "
posiion €, terminal 30.

5. Cutthecable s close s possibi tothe catielug
and stip o 4 - 5 mm of the nsulaton.

5. Crimp e tick yellow 4.0 mn? cable and a new
Section of tin yeliow 0.5 e cable ogelher
tho same cable lug, PIN 91 20 791, Figure .

7. Crimp the other end of the thin yallow 0.§ mm2
catle i the cable ug having part no. 91 20 775,
Figura 4.
Err orao7s

8. Fittho cable lug with he wo cablos oteminal 30 Figure 4. Fittho Cable Lugs (9000)
and ho cable lug withthe thincablototerminal 86
o relay board positon E, Figuro 5.

4. Make sure that he cable ugs snap securely nto
posilon on the relay board

10. Rt the fuse and relay board n tho proteciive
box and insall elay, partno. 85 22 310, a post
tin €. Figuro 8.

11, Check that_the cooling system fan works
properly.

1l Warranty Information:

Forwanantyropais,use Failure Coding 3859-62-0- Figure 5. Fit Jumper o Underside of
01:61. Tima Allowance islabor operaton no, 36501. Folay Board (9000)
s B

Figure 6. Time-Delay Relay, Radiator Fan — 9000




